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Worksheet 1: Raw Glass Substrate Incoming Inspection Standard
· Visual Defect Control: No scratches, bubbles, impurities, surface stains
· Dimension Tolerance for Original Glass Sheets
· Hardness & Light Transmittance Pre-Test Standard
Worksheet 2: CNC Machining Dimensional Tolerance Standard
· Thickness tolerance range ±0.01mm
· Hole position deviation limit ±0.02mm
· Edge chamfer & radius processing standard
· Silk screen positioning tolerance control
Worksheet 3: Vacuum Coating Performance Sampling Test Standard
· AR coating transmittance sampling frequency per production batch
· AF film hydrophobic contact angle test threshold
· Coating adhesion cross-cut test acceptance criteria
· ITO heating layer resistance uniformity test rules
Worksheet 4: Finished Product Final Packing Inspection Standard
· Full appearance recheck for coating peeling, scratches
· Complete optical performance re-sampling test
· Anti-collision foam packaging specification for export shipment
· Batch labeling & traceability code standard for automotive supply chain




The information contained in this document is provided for reference only. Final specifications are subject to mutually approved engineering drawings, production capability review, and customer project requirements.
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