Sheet1 Custom Sapphire Lens Spec Form

	Item
	Required Information
	Fill Example

	1 Product Type
	Half Ball Lens / Ball Lens / Plano-Convex Lens
	Half Ball Lens

	2 Diameter
	Exact dimension + tolerance
	8mm ±0.005mm

	3 Curvature Radius
	R value / focal length
	R4.0mm

	4 Thickness / Center Thickness
	Minimum & max value
	4.0mm

	5 Edge Chamfer
	Yes / No; chamfer size
	Yes, 0.3mm 45°

	6 Optical Coating
	Coating waveband & single/double side
	Double-side AR 1–5μm

	7 Surface Quality
	Scratch/Dig standard
	20/10

	8 Working Environment
	Temperature range, gas corrosion
	-40~300℃ flue gas environment

	9 Batch Requirement
	Prototype / Mass order quantity
	50pcs prototype, 5000pcs monthly mass

	10 Attachment
	CAD / STEP drawing upload
	STEP file attached


Sheet2 Drawing Reminder
Mark all dimensional tolerance on 2D drawing
Indicate optical surface side to avoid machining reversal
Label required spectral band for coating customization
